0.1

0.2 0.3 0.4 0.5 0.6 0.7 0.8 0.9 1.0

3000 4000 5000 6000 8000 9000 10000 11000

Wavelength (Angstroms)

7000

One Shooter

Bilayer Coating

Typical HaO

Monolayer

Typical Front-

Side Illuminated

Device

Quantum Efficiency